Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 62 - LIT-18626-12-93
P. 62

    UF4N10E0.book  Page 55  Tuesday, September 29, 2020  8:02 AM

                            Instrument operation

                            Displaying the time since the last mainte-  EJU45190
                            nance (“Wellness”)                    Engine lock screen “   ”
                            The total number of hours that the engine has  The engine lock  screen shows the  setting
                                                                  screen for the Yamaha Security System in the
                            been running since the last watercraft main-
                                                                  center display. (See page 31 for Yamaha Se-
                            tenance can be displayed.
                                                                  curity System setting procedures.)
                                                                  EJU46400
                                                                  Warning function
                                          Wellness
                                                                  The multifunction information center can indi-
                                  Time Since Last Maintenance     cate the following warnings.
                                                                   Fuel level warning
                                                0Hrs
                                                                   Battery voltage warning
                                            Reset                  Check engine warning
                                                                   Engine overheat warning
                                                                   Oil pressure warning
                                                                   Other warnings (communication errors, ex-
                            To reset the number of hours of operation:  ceeding the maintenance intervals, and so
                            Select “Reset”.                        on)
                            Resetting the settings (“Reset”)      To stop the buzzer when a malfunction is ac-
                            The settings can be reset to their factory de-  tivated, correct the cause of the problem and
                            fault settings. The items that are reset and the  start the engine again, or push the “OK” but-
                            default settings are as follows.      ton of the touchpad control.
                             Display units: US Unit
                             Language: English
                             Trip time: 0.0
                             Distance traveled: 0.0
                             Average fuel consumption per gallon or li-                      1
                              ter: 0.0
                             Total fuel used: 0.0

                                            Reset
                                                                   1 “OK” button
                                       Reset To Factory?          Fuel level warning
                                                                  If the amount of remaining fuel is low, the low-
                                            Reset                 est fuel level segment blinks  orange, “Low

                            To reset the settings:
                            Select “Reset”.

                            55

| 57 58 59 60 61 62 63 64 65 66 67 |