Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - LIT-18626-12-93
P. 49

    UF4N10E0.book  Page 42  Tuesday, September 29, 2020  8:02 AM

                                                                      Watercraft operation

                             Push the “CRUISE/NO WAKE” switch.   When the drive control mode is locked, a PIN
                             Squeeze the throttle lever.         must be entered to operate the drive control
                             Squeeze the RiDE lever.             mode screen.
                            TIP:                                  To select the maximum watercraft speed set-
                            The no-wake mode is also deactivated when  ting:
                            the engine is stopped.                (1) Select “Speed”.
                                                                  (2) Select the maximum  watercraft  speed
                            EJU46380
                            Drive control mode                       setting.
                            The drive control mode is a function for set-
                                                                                   1
                            ting the maximum watercraft speed.
                            The maximum watercraft speed can be se-           Drive Control
                            lected from two settings.                            Speed
                            Activating the drive control mode                    Middle
                            Activation of the drive control mode can be           Low
                            confirmed by the drive control mode indica-
                            tor on  the multifunction information center.
                                                                                  Save
                            When the drive control mode is activated, the
                            drive control mode indicator is shown in light         2
                            yellow.                                1 Maximum watercraft speed setting
                                                                   2 “Save”
                                                    1
                                                                  (3) Select the “Save” button to complete the
                                                                     settings and return to the previous dis-
                                         Drive Control               play.
                                                                  Locking the drive control mode
                                           Speed                  The drive control mode can be locked.
                                                                  To lock the drive control mode:
                                            Lock                  (1) Select “Lock”.
                                                                  (2) Input each digit of the 4-digit PIN, and
                                                                     then push the “OK” button of the touch-
                              1 Drive control mode indicator
                                                                     pad control.
                            To operate the watercraft using the drive con-
                            trol mode:
                            (1) Release the throttle lever and let the en-      Enter PIN
                                gine speed return to idle.                     * * * *
                            (2) Activate each drive control mode.          1       2       3
                            (3) Squeeze the throttle lever.                4       5       6
                            Selecting the drive control mode settings      7       8       9
                            The drive control mode setting for the maxi-
                                                                                   0
                            mum watercraft speed is saved. In addition,
                            the activation and settings of the drive control
                            mode can be locked to prevent others from
                            changing them.

                                                                                                   42

| 44 45 46 47 48 49 50 51 52 53 54 |