Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 53 - LIT-18626-12-93
P. 53

    UF4N10E0.book  Page 46  Tuesday, September 29, 2020  8:02 AM

                                                                     Instrument operation

                            To switch  the speedometer display  units  multifunction information center turns off.
                            (VX-C):                               The speedometer display units change.
                            Start the engine, stop the engine, and then  To switch the  speedometer display  units
                            push the engine stop switch 3 times, pushing  again, repeat this procedure.
                            the switch for 0.4 seconds or more each time,
                            before the  multifunction information center                        2
                            turns  off. The speedometer display  units
                            change.
                            To  switch the speedometer display units
                            again, repeat this procedure.                1

                                                                   1 Clip
                                                                   2 Engine shut-off switch

                                                       1
                              1 Engine stop switch

                                                                                     1
                                                                   1 Speedometer
                                                                  EJU44650
                                                                  Tachometer
                                                                  The tachometer shows the engine speed.
                                                1                                        1
                              1 Speedometer
                            To switch the speedometer display units (VX):
                            Start the engine, stop the engine, and then
                            remove and insert the clip 3 times before the

                                                                   1 Tachometer

                                                                                                   46

| 48 49 50 51 52 53 54 55 56 57 58 |