Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 98 - LIT-18626-12-93
P. 98

    UF4N10E0.book  Page 91  Tuesday, September 29, 2020  8:02 AM

                            Operation

                            watercraft will move in reverse. (See page 36  Operating in neutral
                            for shift system operation procedures.)  When the RiDE lever is squeezed lightly and
                            VX                                    released, the “N” (neutral) shift indicator will
                                         1                        be displayed and the watercraft will stop in its
                                                                  current location. (See page 36 for shift sys-
                                                                  tem operation procedures.)
                                                                  VX
                                                                               1

                              1 “R” (Reverse position)
                            VX DELUXE / VX CRUISER / VX LIMITED

                                                                   1 “N” (Neutral position)
                                                                  VX DELUXE / VX CRUISER / VX LIMITED
                                                    MPH
                                                    RPM

                              14.3V                                                      MPH
                                                           1                             RPM
                              1 “R” (Reverse position)
                                                                   14.3V
                                                                                                1
                                                                   1 “N” (Neutral position)

                            Make sure that there are no obstacles or peo-
                            ple behind you before shifting into reverse.
                            TIP:
                            This model is equipped with a function which
                            limits the engine speed in reverse.

                            91

| 93 94 95 96 97 98 99 100 101 102 103 |