Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - LIT-18626-12-93
P. 42

    UF4N10E0.book  Page 35  Tuesday, September 29, 2020  8:02 AM

                            Control function operation

                            and check the jet intake for clogging. (See
                            page 113 for information on the jet intake.)
                            TIP:
                             It will take about 60 seconds for the water
                              to reach the outlet after the engine is start-
                              ed.
                             Water discharge may not  be  constant
                              when the engine is running at idling speed.
                              If this occurs, apply a little throttle to make
                              sure that water discharges properly.
                            EJU40323
                            Water separator
                            The water separator prevents water from en-
                            tering the fuel tank by collecting any water
                            that has entered the fuel tank breather hose if
                            the watercraft was capsized.
                            If water has collected in the water separator,
                            drain it by loosening the drain screw.

                                                             1

                                                             2

                              1 Water separator
                              2 Drain screw
                            To drain water from the water separator:
                            (1) Place a drain pan or dry cloth under the
                                water separator.
                            (2) Gradually loosen the drain screw to drain
                                the water. Catch the draining water in the
                                drain pan or soak it up with the dry cloth
                                so that it does not spill into the engine
                                compartment. If any water spills into the
                                watercraft, be sure to wipe it up with a
                                dry cloth.
                            (3) Securely tighten the drain screw until it
                                stops.

                            35

| 37 38 39 40 41 42 43 44 45 46 47 |