Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 100 - LIT-18626-12-93
P. 100

    UF4N10E0.book  Page 93  Tuesday, September 29, 2020  8:02 AM

                            Operation

                            (5) Look in  all  directions, start the engine,  (3) Have the first passenger move to the rear
                                and then start off slowly.           of the watercraft.
                            EJU43260
                            Boarding with passenger(s)
                            EWJ01800

                             Severe internal injuries can occur if wa-
                              ter is forced into body cavities as a re-
                              sult of being near the jet thrust nozzle.
                              Do not start the engine until the passen-
                              gers are  seated  with their feet on the
                              floor of the footwell and are securely
                              holding on to the person in front of them
                              or to the handgrip provided.        (4) Have the first passenger board using the
                             Before boarding the watercraft, make   same procedure as the operator, place
                              sure that the engine is stopped. If the  their feet on the floor of the footwell, and
                              engine is running, the reverse gate may  securely hold on to the operator.
                              move down  and a  person boarding
                              could be pinched.

                            The heavier the total weight of the operator
                            and passenger(s), the more difficult it will be
                            to balance the watercraft. Do not operate the
                            watercraft when the total weight exceeds 240
                            kg (530 lb) including any cargo.
                            To board with passenger(s):
                            (1) Board as noted in the previous section
                                “Boarding alone”.                 (5) Have the  second passenger follow the
                                                                     same procedure. When the second pas-
                                                                     senger is boarding, try to  balance  the
                                                                     watercraft together with the first passen-
                                                                     ger.

                            (2) Grip the handlebars with both hands and
                                place both feet on the floor of the foot-
                                well.

                            93

| 95 96 97 98 99 100 101 102 103 104 105 |