Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 75 - LIT-18626-12-93
P. 75

    UF4N10E0.book  Page 68  Tuesday, September 29, 2020  8:02 AM

                                             Operation and handling requirements

                            EJU31823                              Gasohol  containing ethanol can  be used  if
                                    Fuel requirements
                                                                  the ethanol  content  does not exceed 10%
                            EJU45301
                            Fuel                                  and the fuel meets the minimum octane rat-
                            EWJ00283                              ings. E-85 is a fuel blend containing 85% eth-
                                                                  anol and therefore must not be used in this
                             Gasoline and  gasoline vapors are ex-  watercraft.  All ethanol blends  containing
                              tremely flammable. To avoid  fires  and  more than 10% ethanol can cause fuel sys-
                              explosions and to reduce the risk of in-  tem  damage or  engine performance prob-
                              jury when refueling, follow these in-  lems.
                              structions.                         Yamaha does not recommend gasohol con-
                             Gasoline is poisonous and can cause in-  taining methanol because it can cause fuel
                              jury or death. Handle gasoline with care.  system damage  and engine performance
                              Never siphon gasoline by mouth. If you  problems.
                              should swallow some gasoline, inhale a  To fill the fuel tank:
                              lot of gasoline vapor, or get some gaso-  (1) Before refueling, stop the engine. Do not
                              line in your eyes, see your doctor imme-  stand or sit on the watercraft. Never refu-
                              diately. If gasoline spills on  your skin,  el while smoking, or while in the vicinity
                              wash with soap and water. If gasoline  of sparks, open flames, or other sources
                              spills  on your clothing, change  your  of ignition.
                              clothes.                            (2) Place the watercraft in a well-ventilated
                                                                     area and in a horizontal position.
                            ECJ00322
                                                                  (3) Remove the seats, and then check the
                                                                     fuel level. (See page 60 for seat removal
                             Do  not  use leaded gasoline. Leaded
                                                                     and installation procedures.)
                              gasoline can seriously damage the en-
                                                                  (4) Loosen the fuel filler cap and remove it.
                              gine.
                             Avoid getting water and contaminants in
                              the  fuel  tank. Contaminated fuel can
                              cause poor performance  and engine
                              damage. Use only fresh  gasoline that                      1
                              has been stored in clean containers.

                              Recommended fuel:
                                Regular unleaded gasoline with a
                                minimum octane rating of
                                  86
                                   (Pump octane number) = (R + M)/2  1 Fuel filler cap
                                  90 (Research octane number)
                                                                  (5) Slowly add fuel to the fuel tank.
                            Gasohol
                            There are two types of gasohol: gasohol con-
                            taining ethanol and gasohol containing meth-
                            anol.

                                                                                                   68

| 70 71 72 73 74 75 76 77 78 79 80 |