Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - LIT-18626-12-93
P. 44

    UF4N10E0.book  Page 37  Tuesday, September 29, 2020  8:02 AM

                            Watercraft operation

                            VX DELUXE / VX CRUISER / VX LIMITED   VX
                                                                               1

                                                    MPH
                                                    RPM

                              14.3V
                                                           1
                              1 “R” (Reverse position)             1 “N” (Neutral position)
                            To shift into neutral from reverse:   VX DELUXE / VX CRUISER / VX LIMITED
                            Release the RiDE lever. The reverse gate will
                            automatically return to the neutral position
                            and the “N” (neutral) shift indicator will be dis-
                            played.                                                      MPH

                                                                                         RPM
                                          1
                                                                   14.3V
                                                                                                1
                                                                   1 “N” (Neutral position)
                                                                  TIP:
                                                                  Although the neutral position helps keep the
                                                                  watercraft from moving even when the en-
                              1 RiDE lever
                                                                  gine is running, some movement may occur.
                                                                  To shift into forward:
                                                  1               (1) Release the RiDE lever.
                                                                  (2) Squeeze the throttle lever. The reverse
                                                                     gate  will rise completely, the engine
                                                                     speed will increase, the watercraft will

                                                            2

                              1 Reverse gate
                              2 Neutral position

                            37

| 39 40 41 42 43 44 45 46 47 48 49 |