Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 90 - LIT-18626-12-93
P. 90

    UF4N10E0.book  Page 83  Tuesday, September 29, 2020  8:02 AM

                            Pre-operation checks

                            EJU40553                              safe distance away from people, objects,
                            Cooling water pilot outlet check
                            Make sure that water is discharged from the  and other watercraft. [EWJ01860]
                                                                  VX
                            cooling water pilot outlet while the engine is
                            running. (See page 34 for information on the       1                  2
                            cooling water pilot outlet.)
                                                                                                  3
                                                                                                  4

                                                                   1 Shift indicator
                                                                   2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                                                   4 “R” (Reverse position)
                            EJU46240
                            Multifunction information center check
                                                                  VX DELUXE / VX CRUISER / VX LIMITED
                            Make sure that the multifunction information
                            center operates properly. (See page 45, 50
                            for information on proper operation  of the
                            multifunction information center.)
                                                                                         MPH
                            EJU43393
                            Shift system check (VX / VX DELUXE /
                                                                                         RPM
                            VX CRUISER / VX LIMITED)                                     2
                            Operate the throttle lever and RiDE lever, and
                            check that the watercraft moves or does not                  3
                                                                   14.3V
                            move according to the displayed shift indica-                4
                            tor. (See page 36 for shift system operation                        1
                            procedures.)  WARNING! To avoid colli-  1 Shift indicator
                            sions, operate at safe speeds and keep a  2 “F” (Forward position)
                                                                   3 “N” (Neutral position)
                                                                   4 “R” (Reverse position)
                                                                  EJU40172
                                                                  Engine idling speed check
                                                                  Start the engine and warm it up. Use the ta-
                                                                  chometer in the multifunction  information
                                                                  center to make sure  that the engine  idling
                                                                  speed is not significantly above or below the
                                                                  specified range.
                                                                    Engine idling speed:
                                                                      1500 ±100 r/min

                            83

| 85 86 87 88 89 90 91 92 93 94 95 |