Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 102 - LIT-18626-12-93
P. 102

    UF4N10E0.book  Page 95  Tuesday, September 29, 2020  8:02 AM

                            Operation

                            (4) Squeeze the RiDE lever and  move the  (2) Swim to the rear of the watercraft. Turn
                                watercraft back slowly. (See page 36 for  the watercraft over by pulling on the ride
                                RiDE lever operation procedures.)    plate with one hand while pushing down
                            EJU33114                                 on the gunwale with your other hand or
                            Boarding and starting off from a dock
                            (1) Board the watercraft from the side.  your foot.
                            (2) Attach the engine shut-off cord (lanyard)
                                to your left wrist, and then attach the clip
                                to the engine shut-off switch.
                            (3) Push the watercraft away from the dock,
                                grip the handlebars with both hands, and
                                place both feet on the floor of the foot-
                                well.

                            (4) Look in  all  directions, start the engine,
                                and then start off slowly.
                            EJU44210
                            Capsized watercraft                   (3) Start the engine and operate the water-
                            EWJ00672
                                                                     craft at planing speed to drain the bilge
                                                                     water  from the engine  compartment.
                            Improper uprighting can cause injury.    (See page 72 for information on draining
                             Be sure to shut the engine off by pulling  the bilge water. If the engine does not
                              on the engine shut-off cord (lanyard) to  start, see “Towing  the  watercraft” on
                              remove the clip from the engine shut-off  page 115 or “Submerged watercraft” on
                              switch.                                page 115.) NOTICE: Do not run the en-
                             Do not put your hands in the intake    gine at full throttle for at least 1 minute
                              grate.                                 after the engine has been restarted.
                                                                     Bilge  water in  the engine compart-
                            If the watercraft capsizes, turn it over imme-
                                                                     ment can splash into  the  engine,
                            diately.
                                                                     which can result in severe damage.
                            To upright the watercraft:
                            (1) Remove the clip from the engine shut-off  [ECJ00554]
                                switch.

                            95

| 97 98 99 100 101 102 103 104 105 106 107 |