Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 55 - LIT-18626-12-93
P. 55

    UF4N10E0.book  Page 48  Tuesday, September 29, 2020  8:02 AM

                                                                     Instrument operation

                            and have a Yamaha dealer service the water-  blink, and the buzzer sounds intermittently for
                            craft.                                30 seconds.
                                                   1

                              1 Voltmeter
                                                                  If the fuel level warning is activated, refill the
                            EJU37272                              fuel tank as soon as possible. (See page 68
                            Fuel level meter
                                                                  for information on filling the fuel tank.)
                            The fuel level meter shows the amount of fuel
                                                                  After the fuel tank is refilled, the warning sig-
                            remaining in the fuel tank. The amount of re-
                                                                  nals will  be cleared when  the engine  is  re-
                            maining fuel is shown using four display seg-
                                                                  started.
                            ments, which disappear one at a time as the
                                                                  EJU43720
                            fuel level decreases.                 Oil pressure warning
                            TIP:                                  If the oil pressure drops significantly, the oil
                            The accuracy of the fuel level meter varies  pressure warning indicator, the check engine
                            depending on the operating conditions. Use  warning indicator, and the “WARNING” indi-
                            this function as a reference only.    cator light blink, and the buzzer sounds inter-
                                                                  mittently for 30 seconds. At the same time,
                                1                                 the maximum engine speed is limited.

                              1 Fuel level meter
                            EJU44711
                            Fuel level warning                    If the oil pressure warning is activated, imme-
                            If the fuel remaining in the fuel tank drops to
                                                                  diately reduce the engine  speed,  return to
                            about 18 L (4.8 US gal, 4.0 Imp.gal), the low-
                                                                  shore, and then check the engine oil level.
                            est fuel level segment, the fuel level warning
                                                                  (See page 70 for information on checking the
                            indicator, and the “WARNING” indicator light
                                                                  engine oil level.) If the oil level is sufficient,
                                                                  have a Yamaha dealer check the watercraft.
                                                                                                   48

| 50 51 52 53 54 55 56 57 58 59 60 |