Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 72 - LIT-18626-12-93
P. 72

    UF4N10E0.book  Page 65  Tuesday, September 29, 2020  8:02 AM

                            Equipment operation

                            To open the glove compartment:        To close the glove compartment:
                            Pull the  glove  compartment latch up, and  Push the lid down to securely lock it in place.
                            then lift up the lid.

                                                         1

                                                                  To drain water from the glove compartment:
                              1 Glove compartment latch
                                                                  (1) Remove the drain plug on the bottom of
                                                                     the glove compartment to drain the wa-
                                                                     ter.

                                                                                                  1

                                                     1

                              1 Glove compartment

                              Glove compartment:
                                Capacity:                          1 Drain plug
                                  16.5 L (4.4 US gal, 3.6 Imp.gal)  (2) Securely install the drain plug in it original
                                Load limit:                          position.
                                  1.5 kg (3 lb)
                                                                  EJU46011
                                                                  Seat storage compartment
                                                                  The seat storage compartment is located un-
                                                                  der the rear seat.
                                                                  The storage compartment is removable.
                                                                  To open the seat storage compartment:
                                                                  (1) Remove the rear seat. (See page 60 for
                                                                     seat  removal and installation proce-
                                                                     dures.)

                            65

| 67 68 69 70 71 72 73 74 75 76 77 |