Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 40 - LIT-18626-12-93
P. 40

    UF4N10E0.book  Page 33  Tuesday, September 29, 2020  8:02 AM

                            Control function operation

                            Insert the clip  under the engine  shut-off  in 5 seconds, release the start switch, wait 15
                            switch before starting the engine.    seconds, and then try again. NOTICE: Never
                                                                  push the start switch while the engine is
                                                                  running. Do not operate the start switch
                                                         1
                                                                  for  more than 5  seconds, otherwise  the
                                                                  battery will be discharged and the engine
                                                                  will not start. Also, the starter motor could
                                                                  be damaged. [ECJ01041]

                                                           2                             1
                                                        3
                              1 Engine shut-off switch                              START
                              2 Clip
                              3 Engine shut-off cord (lanyard)
                            When the engine is not running, remove the
                            clip from the engine shut-off switch to pre-
                            vent accidental starting or unauthorized op-
                            eration by children or others.         1 Start switch
                                                                  The engine will not start under any of the fol-
                                                                  lowing conditions:
                                                                   Clip is removed from the engine shut-off
                                                                   switch.
                                                                   Throttle lever is squeezed.
                                                                   Throttle lever is malfunctioning.
                                                                  EJU31212
                                                                  Throttle lever
                                                                  The throttle lever increases the engine speed
                                                                  when the lever is squeezed.
                            EJU46190
                            Start switch “  ” (VX-C)                            1
                            ECJ01311

                            Do not run the engine over 4000 r/min on
                            land. Also, do not run the engine for more
                            than 15 seconds without supplying water,
                            otherwise the engine could overheat.

                            The start switch (green button) starts the en-
                            gine when the switch is pushed.        1 Throttle lever
                            Release the start switch as soon as the en-
                                                                  The throttle lever returns automatically to its
                            gine starts to run. If the engine does not start
                                                                  fully closed (idle) position when released.

                            33

| 35 36 37 38 39 40 41 42 43 44 45 |