Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 47 - LIT-18626-12-93
P. 47

    UF4N10E0.book  Page 40  Tuesday, September 29, 2020  8:02 AM

                                                                      Watercraft operation

                                verse assist indicator is displayed,  the  speeds when the engine is running at idling
                                engine speed will increase. The engine  speed.
                                speed can be adjusted to two levels: +1  This function can be used only when the wa-
                                and +2.                           tercraft is in neutral.
                                                                  Activating and deactivating the T.D.E.
                                                                  The activation of the T.D.E. can be confirmed
                                              1
                                                                  by the T.D.E. indicator on the multifunction
                                                                  information center.
                                                                               2   T.D.E. FORWARD

                                                                               3   T.D.E. REVERSE
                                                                                         MPH
                                                                                         RPM
                              1 RiDE lever                                   T.D.E. FORWARD

                                                                   14.3V
                                                                                   1
                                                                   1 T.D.E. indicator
                                                                   2 Forward operation at a very low speed
                                                                   3 Reverse operation at a very low speed
                                                                  To activate the T.D.E.:
                                                                  (1) Shift into neutral.
                                                    1             (2) Push the  upper side of  the “T.D.E.”
                                                                     switch to move forward at a very  low
                              1 “SPEED ADJUST” switch                speed or push the lower side of the
                                                                     “T.D.E.” switch to move in reverse at a
                            To deactivate the reverse assist:
                                                                     very low speed.
                            Perform one of the following operations. The
                            beeper sounds two times and the reverse as-
                            sist indicator  disappears when the  reverse
                            assist is deactivated.
                             Relax your grip on the RiDE lever.
                             Push the lower side of the “SPEED AD-
                              JUST” switch when the reverse assist level
                              is set to +1.
                             Squeeze the throttle lever.
                                                                             1
                            EJU46280
                            T.D.E. (thrust directional enhancer)
                            The T.D.E. is a function for slightly lifting or  1 “T.D.E.” switch
                            lowering the reverse gate from the neutral po-
                            sition  to  operate the watercraft at  very low

                                                                                                   40

| 42 43 44 45 46 47 48 49 50 51 52 |