Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 51 - LIT-18626-12-93
P. 51

    UF4N10E0.book  Page 44  Tuesday, September 29, 2020  8:02 AM

                                                                      Watercraft operation

                                changed in the range of the cruise assist
                                levels –5 to +5.

                                                    1

                              1 “SPEED ADJUST” switch
                            TIP:
                            Because the cruise assist can only be set be-
                            tween engine speeds of approximately 4000
                            r/min  and approximately 7000  r/min, the
                            cruise assist level cannot be adjusted to an
                            engine speed outside of this range.
                            To deactivate the cruise assist:
                            Relax your grip on the throttle lever past the
                            position at which the cruise assist was set.
                            The beeper sounds two times and the cruise
                            assist indicator disappears when the cruise
                            assist is deactivated.

                                                                                                   44

| 46 47 48 49 50 51 52 53 54 55 56 |