Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 115 - LIT-18626-12-93
P. 115

    UF4N10E0.book  Page 108  Tuesday, September 29, 2020  8:02 AM

                                                                                Specifications

                            EJU46440                                Valve clearance-exhaust (cold):
                                      Specifications                  0.26–0.32 mm (0.0102–0.0126 in)
                            Watercraft capacity:                    Lubrication system:
                              Maximum people on board:                Dry sump
                                3 person                            Cooling system:
                              Maximum load capacity:                  Water
                                240 kg (530 lb)                     Starting system:
                            Dimensions and weight:                    Electric
                              Length:                               Ignition system:
                                3.33 m (131.1 in) (VX-C)              T.C.I.
                                3.37 m (132.7 in) (VX LIMITED, VX CRUISER,   Spark plug (NGK):
                                VX DELUXE, VX)                        CR9EB
                              Width:                                Spark plug gap:
                                1.24 m (48.8 in)                      0.7–0.8 mm (0.028–0.031 in)
                              Height:                               Battery capacity:
                                1.20 m (47.2 in)                      12 V, 18 Ah
                              Dry weight:                           Battery type:
                                306 kg (675 lb) (VX DELUXE)           YTX20L-BS
                                308 kg (679 lb) (VX CRUISER)        Charging system:
                                314 kg (692 lb) (VX DELUXE with audio)  Flywheel magneto
                                316 kg (697 lb) (VX LIMITED, VX CRUISER   Drive unit:
                                with audio)                         Propulsion system:
                                318 kg (701 lb) (VX-C)                Jet pump
                                326 kg (719 lb) (VX)                Jet pump type:
                            Performance:                              Axial flow, single stage
                              Maximum fuel consumption:             Impeller rotation:
                                29.1 L/h (7.7 US gal/h, 6.4 Imp.gal/h) (VX-C)  Counterclockwise
                                33.0 L/h (8.7 US gal/h, 7.3 Imp.gal/h) (VX   Jet thrust nozzle angle:
                                LIMITED, VX CRUISER, VX DELUXE, VX)   24+24 °
                              Cruising range at full throttle:    Fuel and oil:
                                2.12 hour (VX LIMITED, VX CRUISER,   Recommended fuel:
                                VX DELUXE, VX)                        Regular unleaded gasoline
                                2.41 hour (VX-C)                    Minimum octane rating (PON):
                              Trolling speed:                         86
                                1500 ±100 r/min                     Minimum octane rating (RON):
                            Engine:                                   90
                              Engine type:                          Recommended engine oil:
                                Liquid cooled 4-stroke, DOHC          YAMALUBE 4W or 4-stroke motor oil
                              Number of cylinders:
                                3
                              Engine displacement:
                                1049 cm³
                              Bore × stroke:                        Recommended engine oil type SAE:
                                82.0 × 66.2 mm (3.23 × 2.61 in)       SAE 10W-30, 10W-40, 20W-40, 20W-50
                              Compression ratio:                    Recommended engine oil grade API:
                                11.0 : 1                              API SG, SH, SJ, SL
                              Valve clearance-intake (cold):        Fuel tank total capacity:
                                0.15–0.22 mm (0.0059–0.0087 in)       70 L (18.5 US gal, 15.4 Imp.gal)

                                                                                                 108

| 110 111 112 113 114 115 116 117 118 119 120 |