Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - LIT-18626-12-93
P. 46

    UF4N10E0.book  Page 39  Tuesday, September 29, 2020  8:02 AM

                            Watercraft operation

                            (2) Lightly squeeze and release the RiDE le-  EJU40003
                                                                   Watercraft operation modes
                                ver. The “N” (neutral) shift indicator will
                                be displayed.                      (VX DELUXE / VX CRUISER /
                                                                            VX LIMITED)

                                                                  EJU45891
                                                                  Reverse assist
                                                                  The reverse assist is a function for temporar-
                                                                  ily increasing the engine speed when moving
                                                                  in  reverse,  such as to  enter the water
                                                                  smoothly when launching the watercraft from
                                                                  a trailer.
                                                                  This function operates  after the engine is
                                                                  started and only if the watercraft is not shifted
                            VX
                                                                  into forward.
                                         1
                                                                  TIP:
                                                                  Once the watercraft is shifted into forward af-
                                                                  ter the engine is started, the reverse assist
                                                                  cannot be operated.
                                                                  Activating and deactivating the reverse
                                                                  assist
                                                                  The activation of the reverse assist can be
                                                                  confirmed by the reverse assist indicator on
                                                                  the multifunction information center.
                              1 “N” (Neutral position)
                            VX DELUXE / VX CRUISER / VX LIMITED

                                                                                         MPH
                                                                                         RPM
                                                    MPH
                                                                            Reverse Assist  +2
                                                    RPM
                                                                   14.3V
                                                                                 1       2
                              14.3V
                                                                   1 Reverse assist indicator
                                                           1       2 Reverse assist level
                              1 “N” (Neutral position)            To activate the reverse assist:
                                                                  (1) Start the engine.
                            TIP:
                                                                  (2) Squeeze the RiDE lever to the fully open
                            If the RiDE lever is squeezed continuously,
                                                                     position, and then push the upper side of
                            the reverse gate will move to the reverse po-
                                                                     the “SPEED ADJUST” switch. Once the
                            sition.
                                                                     beeper sounds three times and the re-
                            39

| 41 42 43 44 45 46 47 48 49 50 51 |