Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 88 - LIT-18626-12-93
P. 88

    UF4N10E0.book  Page 81  Tuesday, September 29, 2020  8:02 AM

                            Pre-operation checks

                            To check the operation of the switches (VX /  EJU32535
                                                                  Fire extinguisher check
                            VX DELUXE / VX CRUISER / VX LIMITED):
                                                                  Check that there is a full fire extinguisher on
                            (1) VX DELUXE /   VX CRUISER /   VX
                                                                  board.
                                LIMITED: If the lock mode is selected for
                                the Yamaha Security System setting, se-
                                lect the unlock mode. (See page 31 for
                                Yamaha Security System setting proce-
                                dures.)
                            (2) Push the engine start/stop switch  to
                                make sure that the engine starts.
                            (3) As soon as the  engine  starts  running,
                                push  the engine start/stop  switch to
                                make sure that the engine stops immedi-
                                ately.
                                                                  To check the fire  extinguisher, see  the  in-
                            (4) Restart the engine, and then pull the en-
                                                                  structions supplied by the fire extinguisher
                                gine shut-off cord (lanyard) to  remove
                                                                  manufacturer. Always keep the fire extin-
                                the clip from the engine shut-off switch
                                                                  guisher secured in the holder with its cover in
                                to make sure that the engine stops im-
                                                                  place.
                                mediately.
                                                                  Always carry a fire extinguisher on board. A
                            EJU40102
                            Storage compartment checks            fire extinguisher is not  standard  equipment
                            Make  sure that  the storage compartments  with this watercraft. If you do not have one,
                            are not damaged and that water has not col-  contact a Yamaha dealer or a fire extinguish-
                            lected in the compartments. (See page 63 for  er dealer to obtain one meeting the proper
                            information on the storage compartments.)  specifications.
                            EJU43800
                            Fire extinguisher holder, cover, and band   Fire extinguisher:
                            checks                                    Classification:
                            Make sure that the fire extinguisher holder,  5-B (B-1)
                            cover, and band are not damaged and that  Capacity:
                            the fire extinguisher is securely held in place  2 lb or more
                            using the band. (See page 66 for information
                                                                  EJU40122
                            on the fire extinguisher holder, cover, and  Safety equipment check
                            band.)                                Check that safety equipment meeting the ap-
                                                                  plicable regulations is on board.
                                                                  EJU32353
                                                                  Hull and deck check
                                                                  Check the hull and deck for damage or other
                                                                  problem.

                            81

| 83 84 85 86 87 88 89 90 91 92 93 |