Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 52 - LIT-18626-12-93
P. 52

    UF4N10E0.book  Page 45  Tuesday, September 29, 2020  8:02 AM

                            Instrument operation

                            EJU44571                              EJU35027
                                Multifunction information         Information display
                                    center (VX-C / VX)            The information display shows watercraft op-
                                                                  erating conditions.
                            The multifunction information center displays
                            various watercraft information.           1        2 3 4     5    6
                                             1             2

                                                                                     8        7
                                                                   1 Fuel level meter
                                                                   2 Shift indicator (VX)
                              1 Information display
                                                                   3 Engine overheat warning indicator
                              2 “WARNING” indicator light
                                                                   4 Check engine warning indicator
                            Multifunction information center initial op-  5 Tachometer / hour meter / voltmeter
                            eration                                6 Oil pressure warning indicator
                            When the multifunction information center is  7 Fuel level warning indicator
                            activated, all of the display segments come  8 Speedometer
                            on. After 2 seconds, the warning indicators in  EJU46430
                            the information display go off, and then the  Speedometer
                            center starts to operate normally.    The speedometer shows the watercraft
                            Multifunction information center standby   speed.
                            state
                            If the  multifunction information center  does
                            not receive any operation input within 30 sec-
                            onds after the engine stops, the center will
                            turn off and enter a standby state. When the
                            engine is started again, the displays return to
                            their state before the center turned off, and
                            then the center starts to operate normally.
                                                                                     1
                                                                   1 Speedometer
                                                                  By switching the display units, the speed can
                                                                  be shown in kilometers per hour “km/h” or
                                                                  miles per hour “MPH”.
                                                                  TIP:
                                                                  “MPH” is selected as the display unit at the
                                                                  Yamaha factory.

                            45

| 47 48 49 50 51 52 53 54 55 56 57 |