Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 50 - LIT-18626-12-93
P. 50

    UF4N10E0.book  Page 43  Tuesday, September 29, 2020  8:02 AM

                            Watercraft operation

                            To unlock the drive control mode:        “CRUISE/NO WAKE” switch. Once  the
                            (1) Select the drive control mode indicator.  beeper sounds three times and the
                            (2) Input each digit of the 4-digit PIN, and  cruise assist indicator is displayed, the
                                then push the “OK” button of the touch-  cruise assist is activated.
                                pad control.
                            (3) Select “Lock”.
                            EJU46390
                            Cruise assist
                            The cruise assist is a function for maintaining
                            a desired engine speed within a fixed range
                            while  operating the watercraft.  Once the
                            cruise  assist  is activated, the set engine
                            speed can be increased or decreased. How-
                            ever, the adjustment is limited to a maximum                      1
                            of five increments above or below the initial  1 “CRUISE/NO WAKE” switch
                            cruise assist setting.
                                                                  (3) When the cruise assist is activated, slow-
                            TIP:                                     ly  squeeze the  throttle lever to  keep it
                            The cruise assist can only be set between en-  squeezed further than the position at
                            gine speeds of approximately 4000 r/min and  which the cruise assist was set.
                            approximately 7000 r/min.
                                                                  TIP:
                            Activating and deactivating the cruise as-
                            sist                                  Check the multifunction information center to
                            Activation of the cruise assist can be con-  make sure that the cruise assist is activated
                            firmed by the cruise assist indicator on the  before squeezing the throttle lever to the full
                            multifunction information center.     throttle position. If the cruise assist is not ac-
                                                                  tivated, the engine will respond normally to
                                                                  the throttle operation.
                                                                  (4) Once the cruise assist is activated, push
                                                                     the upper side of the “SPEED ADJUST”
                                                    MPH
                                                                     switch to increase the set engine speed
                                                                     or the  lower side of the  “SPEED AD-
                                                    RPM
                                       Cruise Assist  +4             JUST” switch to decrease the set engine
                                                                     speed. The engine  speed can  be
                              14.3V
                                            1      2
                              1 Cruise assist indicator
                              2 Cruise assist level
                            To activate the cruise assist:
                            (1) Operate the throttle lever until the de-
                                sired engine speed is reached.
                            (2) When the engine speed reaches the de-
                                sired cruise assist  setting, push the

                            43

| 45 46 47 48 49 50 51 52 53 54 55 |