Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 74 - LIT-18626-12-93
P. 74

    UF4N10E0.book  Page 67  Tuesday, September 29, 2020  8:02 AM

                            Equipment operation

                            To use the fire extinguisher holder and cover:  hood is securely closed before using the
                            (1) Pull the hood latch rearward, and then lift  watercraft.
                                up the rear of the hood.

                                                            1

                              1 Hood latch
                            (2) Unhook the band and remove the fire ex-
                                tinguisher from the fire extinguisher cov-
                                er.

                                      1

                                                          2

                              1 Fire extinguisher holder and cover
                              2 Band
                            (3) Place the fire extinguisher in the fire ex-
                                tinguisher cover, and then securely fas-
                                ten the fire extinguisher with the band.
                            (4) Push the rear of the hood down to se-
                                curely lock it in place. Make sure that the

                            67

| 69 70 71 72 73 74 75 76 77 78 79 |