Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 38 - LIT-18626-12-93
P. 38

    UF4N10E0.book  Page 31  Tuesday, September 29, 2020  8:02 AM

                            Control function operation

                            EJU31027                              (2) Select the lock or unlock mode indicator
                              Watercraft control functions
                                                                     on the multifunction information center.
                            EJU45091
                            Yamaha Security System                (3) Input each digit of the 4-digit PIN, and
                            (VX DELUXE / VX CRUISER / VX             then push the “OK” button of the touch-
                            LIMITED)                                 pad control.
                            The  Yamaha  Security System functions to
                            help prevent unauthorized use or theft of the
                                                                                Enter PIN
                            watercraft. The lock and unlock modes of the
                            security system can  be selected  using  the       * * * *
                            engine lock screen of the multifunction infor-  1      2       3
                            mation center. The engine cannot be started    4       5       6
                            if the lock mode of the security system is se-  7      8       9
                            lected. The engine can only be started if the          0
                            unlock mode is selected.
                            TIP:
                            The  Yamaha Security  System setting  can  TIP:
                            only be selected while the engine is stopped.  The default setting for the PIN is “1234”. The
                            EJU45870                              PIN can also be changed. (See page 54 for in-
                            Yamaha Security System setting        formation on changing the PIN.)
                            The Yamaha Security System setting can be
                                                                  (4) To select the lock mode of the Yamaha
                            confirmed by the lock or unlock mode indica-
                                                                     Security System, select “ON”. To select
                            tor on the multifunction information center.
                                                                     the unlock mode, select “OFF”.
                                                           1
                                                                              Engine Lock

                                                                                  ON
                                                           2
                                                                                  OFF

                              1 Lock mode indicator
                              2 Unlock mode indicator             (5) The beeper sounds once when the lock
                                                                     mode of the Yamaha Security System is
                            To  select the lock or unlock mode of the
                                                                     selected, and two times when the unlock
                            Yamaha Security System:
                                                                     mode is selected.
                            (1) Stop the engine.
                            TIP:
                            The multifunction information center is turned
                            on, even if the engine start/stop switch is also
                            pushed briefly.

                            31

| 33 34 35 36 37 38 39 40 41 42 43 |