Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 112 - LIT-18626-12-93
P. 112

    UF4N10E0.book  Page 105  Tuesday, September 29, 2020  8:02 AM

                            Maintenance

                            EJU43102
                            Periodic maintenance chart
                            The periodic maintenance chart gives general guidelines for periodic maintenance. Have a
                            Yamaha dealer perform the checks in the following chart. However, maintenance may need
                            to be performed more frequently depending on your operating conditions. If you have any
                            questions, consult a Yamaha dealer.
                            This “√” mark indicates items to be checked and serviced by a Yamaha dealer.
                                                                   Initial    Thereafter every
                                                                                   100    200
                                                                         50 hours
                                   Item             Operation              or 12   hours or  hours or   Page
                                                                  10 hours         12      24
                                                                          months   months  months
                                                                            *1
                                                                                   *1      *1
                                              Check fuel hoses and
                             Fuel line                                              √            —
                                              clamps
                             Fuel filler cap/Wa-  Check O-rings for cracks          √
                             ter separator    and deformation                                    —
                                              Check installation and
                             Fuel tank                                              √            —
                                              straps
                                              Check for clogs and dam-
                             Water inlet strainer                                   √            —
                                              age
                                              Check for damage and
                             Cooling water hos-  leakage, and check                 √            —
                             es
                                              clamps
                             Engine oil       Replace                √              √            107
                             Oil filter       Replace                               √            107
                             Intermediate hous-                                     √
                             ing              Lubricate                                          —
                             Spark plugs      Check                  √              √            —
                                              Check state of charge,
                             Battery                                                √            —
                                              terminals and bands
                             Battery leads    Check terminals                       √            —
                                              Check operation and for
                             Steering master                         √              √            —
                                              looseness
                                              Check exterior and con-
                             Steering cable                                         √            —
                                              nections, and lubricate
                             Shift rod and re-
                             verse gate (VX /
                             VX DELUXE /      Check exterior and con-               √            —
                             VX CRUISER / VX   nections, and lubricate
                             LIMITED)
                                              Check for damage and
                             Air filter element                                     √            —
                                              dirt
                                              Check for damage, and
                             Air intake hoses                                       √            —
                                              check clamps
                             Throttle body    Lubricate throttle valve              √            —

                            105

| 107 108 109 110 111 112 113 114 115 116 117 |