Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 85 - LIT-18626-12-93
P. 85

    UF4N10E0.book  Page 78  Tuesday, September 29, 2020  8:02 AM

                                                                    Pre-operation checks

                            EJU40182                              EJU32486
                            Engine unit check                     Battery checks
                            Check the exterior of the engine unit for dam-  Make sure that the battery terminals are not
                            age or other problem.                 damaged and that the battery leads are con-
                            EJU41561                              nected properly. WARNING! Never operate
                            Engine oil level check
                            Make sure that the engine oil level is between  the watercraft if the battery does not have
                                                                  sufficient power to start the engine or if it
                            the minimum and maximum level marks on
                                                                  shows any other signs of decreased pow-
                            the dipstick attached to the oil tank filler cap.
                                                                  er. Loss of battery power may leave you
                            (See page 70 for information on checking the
                                                                  stranded. [EWJ01241]
                            engine oil level.)
                                                                   1
                                                                                 2
                                                       1

                                                                   1 Negative (–) battery terminal: Black lead
                              1 Oil tank filler cap/Dipstick
                                                                   2 Positive (+) battery terminal: Red lead
                                                                  Make sure that the battery is securely held in
                                                                  place.
                                                                  EJU32614
                                                                  Steering system checks
                                                                  Turn the handlebars to the right and left sev-
                                                                  eral times  to  make sure that operation is
                                                                  smooth and unrestricted throughout the
                                    1    2      3                 whole range, and that the free play is not ex-
                                                                  cessive.

                              1 Dipstick
                              2 Maximum level mark
                              3 Minimum level mark
                            EJU32456
                            Bilge water check
                            Make sure that no bilge water has collected in
                            the engine compartment. If bilge water has
                            collected in the engine compartment, drain it.
                            (See page 72 for information on draining the
                            bilge water.)

                                                                                                   78

| 80 81 82 83 84 85 86 87 88 89 90 |