Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - LIT-18626-12-93
P. 48

    UF4N10E0.book  Page 41  Tuesday, September 29, 2020  8:02 AM

                            Watercraft operation

                            TIP:                                  Activating and deactivating the no-wake
                                                                  mode
                            While the T.D.E. is activated, the “N” (neutral)
                                                                  The activation of the no-wake mode can be
                            shift indicator will be displayed and “0” will be
                                                                  confirmed by the no-wake mode indicator on
                            displayed on the speedometer.
                                                                  the multifunction information center.
                            To deactivate the T.D.E.:
                            Perform one of the following operations. The
                            T.D.E. indicator disappears and the T.D.E. is
                            deactivated.
                             Squeeze the throttle lever.                                MPH
                             Squeeze the RiDE lever.
                                                                                         RPM
                             Push and  hold  the “CRUISE/NO WAKE”
                                                                               No Wake
                              switch.
                             While moving forward at a very low speed,  14.3V
                              push the lower side of the “T.D.E.” switch.        1
                             While moving in reverse at a very low
                                                                   1 No-wake mode indicator
                              speed, push the upper side of the “T.D.E.”
                                                                  To activate the no-wake mode:
                              switch.
                                                                  (1) Shift into neutral, or release the throttle
                            TIP:
                                                                     lever and let the engine speed return to
                            The T.D.E. is also deactivated when the en-
                                                                     idle.
                            gine is stopped.
                                                                  (2) Push and hold the “CRUISE/NO WAKE”
                            EJU46420
                            No-wake mode                             switch.  Once  the beeper sounds three
                            The no-wake mode is a function that main-  times and the no-wake mode indicator is
                            tains the engine speed at a fixed setting for  displayed, the no-wake mode is activat-
                            operating the watercraft at low speeds.  ed.
                            This function can be used only when the wa-
                            tercraft is in neutral, or when the watercraft is
                            shifted into forward and the engine is operat-
                            ing at idling speed.
                            TIP:
                            If the no-wake mode is activated when the
                            watercraft is in neutral, the watercraft will au-
                            tomatically shift into forward and the water-
                            craft will start moving at a low speed.                           1
                                                                   1 “CRUISE/NO WAKE” switch
                                                                  To deactivate the no-wake mode:
                                                                  Perform one of the following operations. The
                                                                  beeper sounds two times and the no-wake
                                                                  mode indicator  disappears when  the no-
                                                                  wake mode is deactivated.

                            41

| 43 44 45 46 47 48 49 50 51 52 53 |