Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 109 - LIT-18626-12-93
P. 109

    UF4N10E0.book  Page 102  Tuesday, September 29, 2020  8:02 AM

                                                                           Care and storage

                             Steering cable (jet thrust nozzle end)  (2) Remove the plastic tie that is fastening
                                                                     the fuel hose to the holder on the star-
                                                                     board side of the air filter case.
                                                                  (3) Release the hooks on the port side of the
                                                                     air filter case, and remove the air filter
                                                                     case cover.

                                                                                 2
                                                                                                3
                                                                                                4
                             VX / VX DELUXE / VX CRUISER /  VX   1
                              LIMITED: Shift rod (reverse gate end) and                          5
                              ball joint

                                                                   1 Hook
                                                                   2 Air filter case cover
                                                                   3 Fuel hose
                                                                   4 Plastic tie
                                                                   5 Holder
                                                                  (4) Spray a rust inhibitor such as Yamalube
                                                                     Stor-Rite Engine Fogging Oil into the in-
                                                                     take opening for 3 seconds. WARNING!
                                                                     Do not spray flammable rust inhibitor
                            TIP:                                     products on engine surfaces while the
                            Disconnect the shift rod from the ball joint be-  engine is hot. The sprayed substance
                            fore lubricating.                        or propellants could catch fire. [EWJ00262]
                            EJU46350
                            Rustproofing                                          1
                            Rustproofing the hull, deck, and engine
                            Spray metallic parts of the hull, deck, and en-
                            gine with a rust inhibitor such as Yamalube
                            Silicone Protectant & Lubricant.
                            Rustproofing the internal engine compo-
                            nents
                            Rustproof the internal  engine  components
                            with a rust inhibitor such as Yamalube Stor-
                            Rite Engine Fogging Oil.
                            To rustproof the internal engine components:  1 Intake opening
                            (1) Remove the seats. (See page 60 for seat  (5) Place the air filter case cover in its origi-
                                removal and installation procedures.)  nal position, and then fit the hooks onto
                                                                     the cover.

                                                                                                 102

| 104 105 106 107 108 109 110 111 112 113 114 |