Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 78 - LIT-18626-12-93
P. 78

    UF4N10E0.book  Page 71  Tuesday, September 29, 2020  8:02 AM

                            Operation and handling requirements

                            (6) Loosen the oil tank filler cap and remove  (11) Securely install the seats in their original
                                it, and then wipe  the attached dipstick  positions.
                                clean.

                                                       1

                              1 Oil tank filler cap/Dipstick
                            (7) Screw the oil tank filler cap into the filler
                                hole until it stops. Remove the oil tank
                                filler cap again and make sure that the
                                engine oil level is between the minimum
                                and maximum level marks.

                                    1    2      3

                              1 Dipstick
                              2 Maximum level mark
                              3 Minimum level mark
                            (8) If the  engine oil  level is significantly
                                above the maximum level mark, consult
                                a Yamaha dealer. If the engine oil level is
                                below the minimum  level  mark, slowly
                                add engine oil.
                            (9) Repeat steps 6–8 until the engine oil is at
                                the proper level.
                            (10) Securely install the oil tank filler cap and
                                turn it until it stops.

                            71

| 73 74 75 76 77 78 79 80 81 82 83 |