Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 87 - LIT-18626-12-93
P. 87

    UF4N10E0.book  Page 80  Tuesday, September 29, 2020  8:02 AM

                                                                    Pre-operation checks

                            falls off, allowing the watercraft to contin-  VX / VX DELUXE / VX CRUISER / VX
                                                                  LIMITED:
                            ue to run and cause an accident. [EWJ01221]
                                                                  Check the engine start/stop switch and the
                                                                  engine shut-off switch for proper operation.
                                                                  (See page 32 for information on operating
                                                                  each switch.)
                                                                                    1
                                                                                                2

                            EJU46231
                            Switch checks
                            ECJ01311
                                                                                              3
                            Do not run the engine over 4000 r/min on  1 Clip
                            land. Also, do not run the engine for more  2 Engine shut-off switch
                            than 15 seconds without supplying water,  3 Engine shut-off cord (lanyard)
                            otherwise the engine could overheat.

                            VX-C:
                            Check the start switch, the engine stop
                            switch, and  the engine shut-off  switch for
                            proper operation. (See pages 32 to 33 for in-
                            formation on operating each switch.)

                                           1     2     3
                                                                                      1

                                                                   1 Engine start/stop switch
                                                                  To check the operation of the switches (VX-C):
                                       4                          (1) Push the start switch to make sure that
                                                                     the engine starts.
                                          5                       (2) As  soon as the  engine starts running,
                                                                     push the engine stop switch to  make
                              1 Engine shut-off switch               sure that the engine stops immediately.
                              2 Clip                              (3) Restart the engine, and then pull the en-
                              3 Start switch                         gine  shut-off cord (lanyard) to  remove
                              4 Engine stop switch                   the clip from the engine shut-off switch
                              5 Engine shut-off cord (lanyard)
                                                                     to make sure that the engine stops im-
                                                                     mediately.

                                                                                                   80

| 82 83 84 85 86 87 88 89 90 91 92 |