Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 121 - LIT-18626-12-93
P. 121

    UF4N10E0.book  Page 114  Tuesday, September 29, 2020  8:02 AM

                                                                           Trouble recovery

                                ler, jet pump housing, and jet thrust noz-  (4) Raise the reverse gate to the forward po-
                                zle.                                 sition.
                                If debris is difficult to remove, consult a
                                Yamaha dealer.
                            EJU43472
                            Raising the reverse gate (VX /                            1
                            VX DELUXE / VX CRUISER / VX
                            LIMITED)
                            If the RiDE system malfunctions and the re-                            2
                            verse gate remains in the lowered position,
                            the watercraft will not be able to move for-
                            ward.
                            After raising the reverse gate so that the wa-  1 Reverse gate
                            tercraft can move  forward, immediately  re-  2 Forward position
                            turn to shore and have a  Yamaha dealer
                                                                  TIP:
                            service the watercraft.
                            To raise the reverse gate:             While the shift rod is disconnected, the re-
                            (1) Stop the engine and remove the clip from  verse gate will not move to the neutral po-
                                the engine shut-off switch.        sition or reverse position even if the RiDE
                            (2) Enter the water and move to the rear of  lever is squeezed.
                                the watercraft.                    If the RiDE lever is squeezed while the shift
                            (3) Slide the shift rod joint toward the bow,  rod is disconnected, the watercraft will
                                and then disconnect the shift rod joint  move forward.
                                                                  EJU34642
                                from the ball joint.              Jumping the battery
                                                                  If the watercraft battery has run down, the en-
                                                                  gine can be started using a 12-volt booster
                                                                  battery and jumper cables.
                                                                  EJU34664
                                                                  Connecting the jumper cables
                                                                  EWJ01251
                                                                  To avoid battery explosion  and serious
                                                                  damage to the electrical system:
                                1        2                         Do not reverse the polarity of the jumper
                              1 Shift rod joint                    cables when connecting to the batter-
                              2 Ball joint                         ies.
                                                                   Do not connect the negative (–) jumper
                                                                   cable to the negative (–) terminal of the
                                                                   watercraft battery.
                                                                   Do not touch the positive (+) jumper ca-
                                                                   ble to the negative (–) jumper cable.

                                                                                                 114

| 116 117 118 119 120 121 122 123 124 125 126 |