Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 93 - LIT-18626-12-93
P. 93

    UF4N10E0.book  Page 86  Tuesday, September 29, 2020  8:02 AM

                                                                                      Operation

                                the jet intake, causing impeller dam-  (4) VX-C: With the throttle lever released,
                                age and engine overheating. [ECJ00473]  push the start switch (green button) to
                                                                     start the engine. (See page 33 for infor-
                                                                     mation on operating the start switch.)

                            (3) Attach the engine shut-off cord (lanyard)           START
                                to your left wrist, and then attach the clip
                                to the engine shut-off switch. (See page  VX / VX DELUXE /  VX CRUISER / VX
                                32 for information on operating the en-  LIMITED: With the throttle lever released,
                                gine shut-off switch.) WARNING! Check  push the engine start/stop switch (red
                                that the engine shut-off cord (lanyard)  button) to start the engine. (See page 32
                                is attached  correctly. If the engine  for information on operating the engine
                                shut-off cord (lanyard) is not attached  start/stop switch.)
                                correctly, it may not pull free when the
                                operator falls off, allowing the water-
                                craft to continue to run and cause an
                                accident. [EWJ00582]
                                              1
                                                          2

                                                                  EJU46260
                                                                  Stopping the engine
                                                                  Release the throttle lever, and then push the
                                                        3         engine stop switch (red button) (VX-C) or the
                              1 Clip                              engine  start/stop switch (red  button) (VX /
                              2 Engine shut-off switch            VX DELUXE / VX CRUISER / VX LIMITED) to
                              3 Engine shut-off cord (lanyard)    stop the engine.  WARNING! You  need
                                                                  throttle to  steer. Shutting the engine off
                                                                  can cause you to hit an obstacle you are

                                                                                                   86

| 88 89 90 91 92 93 94 95 96 97 98 |