Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 94 - LIT-18626-12-93
P. 94

    UF4N10E0.book  Page 87  Tuesday, September 29, 2020  8:02 AM

                            Operation

                            attempting to avoid. A collision could re-  EJU44991
                                                                  Operating the watercraft
                            sult in severe injury or death. [EWJ00602]
                                                                  VX-C:
                            VX-C
                                                                  When the  engine is running, the  watercraft
                                                                  will move forward at trolling speed even if the
                                                                  throttle lever is in the fully closed (idle) posi-
                                                                  tion.

                            VX / VX DELUXE / VX CRUISER / VX
                            LIMITED

                                                                  VX / VX DELUXE / VX CRUISER / VX
                                                                  LIMITED:
                                                                  When the throttle lever is squeezed, the “F”
                                                                  (forward) shift indicator will be displayed and
                                                                  the watercraft will move forward. While the
                                                                  “F” (forward) shift indicator is displayed, the
                                                                  watercraft will move forward at trolling speed
                                                                  even if the throttle lever is in the fully closed
                            EJU32873
                            Leaving the watercraft
                            If leaving the watercraft, remove the clip from
                            the  engine shut-off switch  to prevent  acci-
                            dental starting or unauthorized operation by
                            children or others.

                            87

| 89 90 91 92 93 94 95 96 97 98 99 |