Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 71 - LIT-18626-12-93
P. 71

    UF4N10E0.book  Page 64  Tuesday, September 29, 2020  8:02 AM

                                                                     Equipment operation

                            To open the bow storage compartment:  To close the bow storage compartment:
                            Pull the hood latch rearward, and then lift up  Push the rear of the hood down to securely
                            the rear of the hood.                 lock it in place.

                                                            1

                              1 Hood latch                        EJU46211
                                                                  Glove compartment
                                                                  The glove compartment is located in front of
                                             1                    the seat.
                                                                  TIP:
                                                                   Make sure the seal of lid is intact, clear and
                                                                   properly positioned before using.
                                                                   Make sure the seals around the USB char-
                                                                   ger and 12V DC outlet are intact and prop-
                                                                   erly positioned before using.
                                                                   Completely dry inside of  the glove com-
                              1 Bow storage compartment            partment and its contents before and after
                                                                   using.
                              Bow storage compartment:             Make sure nothing is pinches between the
                                Capacity:
                                  92.0 L (24.3 US gal, 20.2 Imp.gal)  glove compartment and the lid when clos-
                                Load limit:                        ing the glove compartment.
                                  5.0 kg (11 lb)                   When not in use, the rubber caps for the
                                                                   USB charger and 12V DC outlet should be
                                                                   installed to cover the connectors.

                                                                                                   64

| 66 67 68 69 70 71 72 73 74 75 76 |