Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 54 - LIT-18626-12-93
P. 54

    UF4N10E0.book  Page 47  Tuesday, September 29, 2020  8:02 AM

                            Instrument operation

                            TIP:                                  TIP:
                            While the engine is stopped, the battery volt-  If the engine is stopped after the check en-
                            age and the total engine hours are displayed  gine warning is activated, the hour meter and
                            alternately.                          error code will be displayed alternately at 3-
                            EJU46200                              second intervals.
                            Shift indicator (VX)
                            This indicator shows the  reverse gate  shift  Hour meter
                                                                  The hour meter shows the total number of
                            positions: “F” (forward), “N” (neutral), and “R”
                                                                  hours that the engine has been running since
                            (reverse).  (See page 36 for shifting proce-
                                                                  the watercraft was new.
                            dures.)
                                                                                         1
                                         1
                                                             2
                                                             3

                                                             4

                                                                   1 Hour meter
                              1 Shift indicator
                              2 “F” (Forward position)            TIP:
                              3 “N” (Neutral position)            The elapsed time will be kept even if the bat-
                              4 “R” (Reverse position)            tery terminals have been disconnected.
                            EJU44700                              Voltmeter
                            Hour meter and voltmeter
                                                                  The voltmeter shows the battery voltage.
                            The hour meter and voltmeter are displayed
                                                                  When the battery voltage is normal, the volt-
                            in the tachometer portion of the information
                                                                  meter displays approximately 12 volts.
                            display while the engine is stopped.
                                                                  If the battery voltage has dropped significant-
                            The hour meter and voltmeter are displayed
                                                                  ly, “Lo” is displayed on the voltmeter, and all
                            alternately at 3-second intervals.
                                                                  other display segments  of the information
                                                   1              display turn off. If the battery voltage has ris-
                                                                  en significantly, “HI” is displayed. If “Lo” or
                                                                  “HI” is displayed, immediately return to shore

                              1 Hour meter and voltmeter

                            47

| 49 50 51 52 53 54 55 56 57 58 59 |