Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 110 - LIT-18626-12-93
P. 110

    UF4N10E0.book  Page 103  Tuesday, September 29, 2020  8:02 AM

                            Care and storage

                            TIP:
                            Make sure that the air filter case cover is se-
                            curely installed.
                            (6) Fasten the fuel hose to the holder using
                                the plastic tie.
                            (7) Make sure that the area around the wa-
                                tercraft is clear, and then start the engine
                                in a well-ventilated area and let it run at
                                idle for 15 seconds. (See page 33 for in-
                                formation on starting the engine.)
                            (8) Stop the engine.
                            (9) Securely install the seats in their original
                                positions.

                            103

| 105 106 107 108 109 110 111 112 113 114 115 |