Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 23 - LIT-18626-12-93
P. 23

    UF4N10E0.book  Page 16  Tuesday, September 29, 2020  8:02 AM

                                                                         Safety information

                            EJU30831                              EJU44610
                               Recommended equipment                    Hazard information
                            The following items  should be carried on   Never start the engine or let it run for any
                            board your watercraft:                 length of time in an enclosed area. Exhaust
                             Sound-signaling device               fumes contain carbon monoxide, a color-
                              You should carry a whistle or other sound-  less, odorless gas that may cause loss of
                              signaling device that can be used to signal  consciousness and death within a short
                              other boats. See “Rules of the Road” for  time. Always operate the watercraft in an
                              more information.                    open area.
                             Visual distress signals              Do not touch the hot oil tank, muffler, or en-
                              It is recommended that a U.S. Coast Guard  gine during or immediately after engine op-
                              approved pyrotechnic device be stored in a  eration; they can cause serious burns.
                              waterproof container on your watercraft. A   Do  not place  magnets or objects  with a
                              mirror can also be used as an emergency  strong magnetic force near the throttle le-
                              signal. Contact a  Yamaha  dealer or the  ver or RiDE lever (VX / VX DELUXE /
                              U.S. Coast Guard for more information.  VX CRUISER / VX LIMITED). The electronic
                             Watch                                throttle mechanism of the levers can be ad-
                              A watch is  helpful so you will know how  versely affected, which could cause loss of
                              long you have been operating the water-  control. In addition, do not place objects
                              craft.                               susceptible to magnetic forces (i.e., credit
                             Towline                              cards, watches, etc.) close to the throttle
                              A towline can be used to tow a disabled  lever or RiDE lever.
                              watercraft in an emergency.

                                                                                                   16

| 18 19 20 21 22 23 24 25 26 27 28 |