Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 86 - LIT-18626-12-93
P. 86

    UF4N10E0.book  Page 79  Tuesday, September 29, 2020  8:02 AM

                            Pre-operation checks

                            Turn the handlebars as far as possible to the  lever returns automatically to its fully closed
                            right and left to make sure that the jet thrust  position when released.
                            nozzle moves as the handlebars are turned,
                            and that there is no difference between the
                            right and left fully turned positions of the jet
                            thrust nozzle.

                                                                  EJU42181
                                                                  Throttle lever checks
                                                                  Operate the throttle lever several times to
                                                                  make sure that operation is smooth through-
                                                                  out the whole range. Also, make sure that the
                                                                  throttle lever returns automatically to its fully
                                                                  closed (idle) position when released.

                              Difference between fully turned posi-
                              tions of jet thrust nozzle (distances A
                              and B):
                                                                  EJU45351
                                Maximum 5 mm (0.20 in)            Yamaha Security System check
                                                                  (VX DELUXE / VX CRUISER / VX LIMITED)
                            EJU43213                              Make sure that the Yamaha Security System
                            RiDE lever checks (VX / VX DELUXE /
                                                                  operates properly. (See page 31 for Yamaha
                            VX CRUISER / VX LIMITED)
                            Operate the RiDE lever several times to make  Security System setting procedures.)
                                                                  EJU32664
                            sure that operation is smooth throughout the  Engine shut-off cord (lanyard) check
                            whole range. Also, make sure that the RiDE  Make sure that the engine shut-off cord (lan-
                                                                  yard) is not damaged. If the cord is damaged,
                                                                  replace it.  WARNING! Never try to repair
                                                                  the engine shut-off cord (lanyard) or tie it
                                                                  together. The  engine  shut-off cord (lan-
                                                                  yard) may not pull free when the operator

                            79

| 81 82 83 84 85 86 87 88 89 90 91 |