Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 57 - LIT-18626-12-93
P. 57

    UF4N10E0.book  Page 50  Tuesday, September 29, 2020  8:02 AM

                                                                     Instrument operation

                            the hour meter and error code alternately at  EJU45941
                                                                     Multifunction information
                            3-second intervals.
                                                                        center (VX DELUXE /
                                                   1
                                                                    VX CRUISER / VX LIMITED)
                                                                  The multifunction information center displays
                                                                  various watercraft information.
                                                                  The multifunction information center can turn
                                                                  the various functions on or off or change set-
                                                                  tings by using the d-pad of the  touchpad
                                                                  control.
                                                                  In addition, the language and display units
                                                                  shown can be changed. (See page 53 for in-
                              1 Error code
                                                                  formation on changing the language and dis-
                            If the check engine warning is activated, im-  play units.) In the illustrations in this manual,
                            mediately reduce the engine speed, return to  English is used for the language and US units
                            shore, and have a Yamaha dealer check the  are used for the display units.
                            engine.                               Turning on the multifunction information
                                                                  center
                                                                  When the engine start/stop switch is pushed,
                                                                  the multifunction information center turns on.
                                                                  After the logo display appears for a few sec-
                                                                  onds, the home screen is displayed.
                                                                  TIP:
                                                                  The multifunction information center is turned
                                                                  on, even if the engine start/stop switch is also
                                                                  pushed briefly.
                                                                  Turning off the multifunction information
                                                                  center
                                                                  If the multifunction information center does
                                                                  not receive any operation input within 25 sec-
                                                                  onds after the engine stops or if 3 minutes
                                                                  have elapsed after the engine stops, the cen-
                                                                  ter turns off.
                                                                  TIP:
                                                                  The multifunction information center turns off
                                                                  3 minutes after the engine stops even if there
                                                                  is operation input.

                                                                                                   50

| 52 53 54 55 56 57 58 59 60 61 62 |