Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 73 - LIT-18626-12-93
P. 73

    UF4N10E0.book  Page 66  Tuesday, September 29, 2020  8:02 AM

                                                                     Equipment operation

                            (2) Push the latch forward, and then lift up  To close the seat storage compartment:
                                the lid and remove it.            (1) Insert the projections on the lid into the
                                                                     slots on the seat storage compartment.

                                           1
                                                             2

                              1 Lid
                              2 Latch
                                                                  (2) Push the rear of the lid down.

                                                     1

                              1 Seat storage compartment
                                                                  (3) Securely install the rear seat in its original
                              Seat storage compartment:              position.
                                Capacity:                         EJU46030
                                  5.4 L (1.4 US gal, 1.2 Imp.gal)  Fire extinguisher holder and cover
                                Load limit:                       The fire extinguisher holder and cover are lo-
                                  3.0 kg (7 lb)                   cated in the bow storage compartment.

                                                                                                   66

| 68 69 70 71 72 73 74 75 76 77 78 |