Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 59 - LIT-18626-12-93
P. 59

    UF4N10E0.book  Page 52  Tuesday, September 29, 2020  8:02 AM

                                                                     Instrument operation

                            (See page 55 for information about the warn-  TIP:
                            ing descriptions.)                    The accuracy of  the  fuel  level meter varies
                                                         1        depending on the operating conditions. Use
                                                                  this function as a reference only.
                                                                  EJU45151
                                                                  Home screen “ ”
                                                                  The center display of the home screen shows
                                                   MPH
                                                                  the speedometer and the indicators for the
                                                   RPM
                                                                  operation modes. (See page 39 for informa-
                                                                  tion on the functions of the various modes.)
                                14.3V
                                                                  TIP:
                                 2           3           4        If the engine speed increases while the drive
                              1 Fuel level meter
                                                                  control mode screen, setting menu screen, or
                              2 Voltmeter
                                                                  engine lock screen  is  displayed, the  multi-
                              3 Tachometer
                                                                  function information center will automatically
                              4 Shift indicator
                                                                  switch to the home screen.
                            Voltmeter
                            The voltmeter shows  the battery  voltage.             1
                            When the battery voltage is normal, the volt-
                            meter displays approximately 14 volts.
                            If the  battery voltage has dropped or risen                   MPH
                            significantly, the battery voltage warning will
                                                                                          RPM
                            activate and the  voltage display will blink.
                            (See page 56 for information on the battery
                            voltage warning.)
                                                                   2    Reverse Assist  +2
                            Tachometer
                            The tachometer shows the engine speed and  3  T.D.E. FORWARD
                            the number of display segments.
                            Shift indicator                        4    No Wake
                            This indicator shows the  reverse gate  shift  5  Cruise Assist  +4
                            positions: “F” (forward), “N” (neutral), and “R”
                            (reverse).  (See page 36 for shifting proce-  6  Drive Control
                            dures.)                                1 Speedometer
                            Fuel level meter                       2 Reverse assist indicator
                            The fuel level meter shows the amount of fuel  3 T.D.E. indicator
                            remaining in the fuel tank using the number of  4 No-wake mode indicator
                            display segments.                      5 Cruise assist indicator
                                                                   6 Drive control indicator
                            If the amount of remaining fuel is low, the fuel
                            level warning will activate. (See page 55 for  Speedometer
                            information on the fuel level warning.)  The speedometer shows the watercraft
                                                                  speed.

                                                                                                   52

| 54 55 56 57 58 59 60 61 62 63 64 |