Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 62 - LIT-18626-13-05
P. 62

    UF4P11E0.book  Page 56  Friday, October 30, 2020  9:39 AM

                            Equipment operation

                            when released. WARNING! Do not use the  towing it in an emergency. (See page 105 for
                            reboarding step to lift the watercraft. The  information on towing the watercraft.)
                            reboarding step is not designed to support
                            the watercraft’s weight. If the reboarding
                            step  breaks,  the watercraft could fall,
                            which could result in severe injury. [EWJ01212]

                                        1

                                                                     1
                                                                   1 Bow eye
                                                                  EJU34882
                                                                  Stern eyes
                                                                  The stern eyes are used to attach a rope to
                                                                  the watercraft when transporting or mooring
                              1 Reboarding step                   it.

                                                                                   1
                                                                   1 Stern eye
                            ECJ00743
                                                                  EJU40423
                                                                  Cleat
                            Use the reboarding step only to board the  The cleat is used to attach a ski rope to the
                            watercraft in the water. Do not use the re-  watercraft  when pulling a wakeboarder or
                            boarding step for any other purpose. The  water-skier.  WARNING! Do not use the
                            watercraft can be damaged.            cleat to lift the watercraft. The cleat is not
                                                                  designed to support the watercraft’s
                            EJU34873
                            Bow eye                               weight. If the cleat breaks, the watercraft
                            The bow eye is used to attach a rope to the
                            watercraft when transporting, mooring, or

                            56

| 57 58 59 60 61 62 63 64 65 66 67 |