Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 69 - LIT-18626-13-05
P. 69

    UF4P11E0.book  Page 63  Friday, October 30, 2020  9:39 AM

                                             Operation and handling requirements

                            EJU40291                              Yamalube the best choice for your Yamaha
                                 Engine oil requirements
                                                                  engine.
                            EJU41514
                            Engine oil
                            ECJ00282

                            Use only 4-stroke engine oil. Usage of 2-
                            stroke engine oil could result in severe en-
                            gine damage.
                                                                  Checking the engine oil level
                              Recommended engine oil:             EWJ00341
                                YAMALUBE 4W or 4-stroke motor oil
                              Recommended engine oil type:
                                SAE 10W-30, 10W-40, 20W-40,       Engine oil is extremely hot immediately af-
                                20W-50                            ter the engine is turned off. Coming in con-
                              Recommended engine oil grade:       tact with or getting any engine oil on your
                                API SG, SH, SJ, SL
                                                                  clothes could result in burns.

                            TIP:                                  ECJ01002
                            When the engine is operated at high speeds,
                            some engine oil may be consumed. Be sure  Make sure  that debris and  water  do not
                            to check the engine oil level.        enter the oil filler hole. Debris and water in
                            Why Yamalube                          the engine oil can cause serious engine
                            YAMALUBE oil is a Genuine YAMAHA Part  damage.
                            born of the engineers’ passion and belief that
                                                                  To check the engine oil level:
                            engine oil is an important liquid engine com-
                                                                  (1) Place the watercraft in a precisely level
                            ponent. We form teams of specialists in the
                                                                     position  on land with the engine
                            fields of mechanical engineering, chemistry,
                                                                     stopped. If the engine was running, allow
                            electronics and track testing, and have them
                                                                     the engine oil to settle by waiting 5 min-
                            develop the engine together with the oil it will
                                                                     utes or more before checking the oil lev-
                            use. Yamalube oils take full advantage of the
                                                                     el.
                            base oil’s qualities and blend in the ideal bal-
                                                                  (2) Remove the seats. (See page 54 for seat
                            ance of additives to make sure the final oil
                                                                     removal and installation procedures.)
                            clears our performance standards. Thus,
                            Yamalube mineral, semisynthetic and syn-
                            thetic oils have their own distinct characters
                            and value. Yamaha’s experience gained over
                            many years of research  and development
                            into oil since the  1960’s helps make

                                                                                                   63

| 64 65 66 67 68 69 70 71 72 73 74 |