Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - LIT-18626-13-05
P. 48

    UF4P11E0.book  Page 42  Friday, October 30, 2020  9:39 AM

                            Watercraft operation

                            EJU45921                              To select the maximum watercraft speed and
                            Drive control mode
                                                                  acceleration settings:
                            The drive control mode is a function for set-
                                                                  (1) Select “Speed/Acceleration”.
                            ting the maximum watercraft speed and ac-
                                                                  (2) Select the maximum  watercraft  speed
                            celeration for stable towing, and to adjust the
                                                                     setting under “Speed” and the accelera-
                            trim angle automatically.
                                                                     tion setting under “Accel.”
                            The maximum watercraft speed can be se-
                            lected from three settings and the accelera-  1                2
                            tion can be selected from two settings.
                                                                              Drive Control
                            Activating the drive control mode            Speed            Accel.
                            Activation of the drive control mode can be
                                                                         High
                            confirmed by the drive control mode indica-                   Nomal
                                                                         Middle
                            tor on  the multifunction information center.
                                                                         Low              Slow
                            When the drive control mode is activated, the
                            drive control mode indicator is shown in light        Save
                            yellow.
                                                                                   3
                                                    1              1 Maximum watercraft speed setting
                                                                   2 Acceleration setting
                                                                   3 “Save”
                                         Drive Control            (3) Select the “Save” button to complete the
                                                                     settings and return to the previous dis-
                                      Speed/Acceleration
                                                                     play.
                                          Auto Trim               Activating the auto trim
                                                                  The auto trim is activated, the trim angle is
                                            Lock
                                                                  automatically adjusted.
                                                                  When the auto trim is activated, the drive
                              1 Drive control mode indicator
                                                                  control mode indicator and “Auto Trim” are
                            To operate the watercraft using the drive con-
                                                                  shown in light yellow.
                            trol mode:
                            (1) Release the throttle lever and let the en-
                                gine speed return to idle.                    Drive Control
                            (2) Activate each drive control mode.
                            (3) Squeeze the throttle lever.                Speed/Acceleration
                            Selecting the drive control mode settings          Auto Trim
                            The drive control mode settings for the max-
                            imum watercraft speed and acceleration are           Lock
                            saved. In addition, the activation and settings
                            of the drive control mode can be locked to                           1
                            prevent others from changing them.     1 “Auto Trim”
                            When the drive control mode is locked, a PIN
                            must be entered to operate the drive control
                            mode screen.

                            42

| 43 44 45 46 47 48 49 50 51 52 53 |