Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 82 - LIT-18626-13-05
P. 82

    UF4P11E0.book  Page 76  Friday, October 30, 2020  9:39 AM

                            Pre-operation checks

                            tion on the cooling water pilot outlets.)  EJU40172
                                                                  Engine idling speed check
                                                                  Start the engine and warm it up. Use the ta-
                                                                  chometer in the multifunction  information
                                                                  center to make sure  that the engine  idling
                                                                  speed is not significantly above or below the
                                                                  specified range.
                                                                    Engine idling speed:
                                                                      1250 ±100 r/min

                            EJU45260
                            Multifunction information center check
                            Make sure that the multifunction information
                            center operates properly. (See page 45 for in-
                            formation on proper operation of the multi-
                            function information center.)
                            EJU43393
                            Shift system check
                            Operate the throttle lever and RiDE lever, and
                            check that the watercraft moves or does not
                            move according to the displayed shift indica-
                            tor. (See page 35 for shift system operation
                            procedures.)  WARNING! To avoid colli-
                            sions, operate at safe speeds and keep a
                            safe distance away from people, objects,
                            and other watercraft. [EWJ01860]

                                            RPM
                                            x1000
                                                   MPH
                                                    2
                                                    3
                              14.3V
                                                    4
                                                           1
                              1 Shift indicator
                              2 “F” (Forward position)
                              3 “N” (Neutral position)
                              4 “R” (Reverse position)

                            76

| 77 78 79 80 81 82 83 84 85 86 87 |