Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 105 - LIT-18626-13-05
P. 105

    UF4P11E0.book  Page 99  Friday, October 30, 2020  9:39 AM

                                                                                Specifications

                            EJU46440                                Spark plug gap:
                                      Specifications                  0.8–0.9 mm (0.031–0.035 in)
                            Watercraft capacity:                    Battery capacity:
                              Maximum people on board:                12 V, 18 Ah
                                3 person                            Battery type:
                              Maximum load capacity:                  YTX20L-BS
                                240 kg (530 lb)                     Charging system:
                            Dimensions and weight:                    Flywheel magneto
                              Length:                             Drive unit:
                                3.35 m (131.9 in)                   Propulsion system:
                              Width:                                  Jet pump
                                1.24 m (48.8 in)                    Jet pump type:
                              Height:                                 Axial flow, single stage
                                1.20 m (47.2 in)                    Impeller rotation:
                              Dry weight:                             Counterclockwise
                                342 kg (754 lb) (GP1800R SVHO)      Jet thrust nozzle angle:
                                350 kg (772 lb) (GP1800R SVHO with audio)   24+24 °
                            Performance:                            Jet thrust nozzle trim angle:
                              Maximum fuel consumption:               -5, -3, 0, 3, 6 °
                                80.7 L/h (21.3 US gal/h, 17.8 Imp.gal/h)  Fuel and oil:
                              Cruising range at full throttle:      Recommended fuel:
                                0.87 hour                             Premium unleaded gasoline
                              Trolling speed:                       Minimum octane rating (PON):
                                1250 ±100 r/min                       91
                            Engine:                                 Minimum octane rating (RON):
                              Engine type:                            95
                                Liquid cooled 4-stroke, DOHC        Recommended engine oil:
                              Number of cylinders:                    YAMALUBE 4W or 4-stroke motor oil
                                4
                              Engine displacement:
                                1812 cm³
                              Bore × stroke:
                                86.0 × 78.0 mm (3.39 × 3.07 in)     Recommended engine oil type SAE:
                              Compression ratio:                      SAE 10W-30, 10W-40, 20W-40, 20W-50
                                8.5 : 1                             Recommended engine oil grade API:
                              Valve clearance-intake (cold):          API SG, SH, SJ, SL
                                0.14–0.23 mm (0.0055–0.0091 in)     Fuel tank total capacity:
                              Valve clearance-exhaust (cold):         70 L (18.5 US gal, 15.4 Imp.gal)
                                0.36–0.45 mm (0.0142–0.0177 in)     Engine oil quantity with oil filter replacement:
                              Lubrication system:                     3.7 L (3.91 US qt, 3.26 Imp.qt)
                                Wet sump                            Engine oil quantity without oil filter replacement:
                              Cooling system:                         3.5 L (3.70 US qt, 3.08 Imp.qt)
                                Water                               Engine oil total quantity:
                              Starting system:                        5.3 L (5.60 US qt, 4.66 Imp.qt)
                                Electric
                              Ignition system:
                                T.C.I.
                              Spark plug (NGK):
                                LFR7A

                                                                                                   99

| 100 101 102 103 104 105 106 107 108 109 110 |