Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 47 - LIT-18626-13-05
P. 47

    UF4P11E0.book  Page 41  Friday, October 30, 2020  9:39 AM

                                                                      Watercraft operation

                            gine speed each above and below the initial  displayed, the no-wake mode is activat-
                            engine speed.                            ed.
                            This function can be used only when the wa-
                            tercraft is in neutral, or when the watercraft is
                            shifted into forward and the engine is operat-
                            ing at idling speed.
                            TIP:
                            If the no-wake mode is activated when the
                            watercraft is in neutral, the watercraft will au-
                            tomatically shift into forward and the water-
                            craft will start moving at a low speed.                           1
                            Activating and deactivating the no-wake
                                                                   1 “CRUISE/NO WAKE” switch
                            mode
                            The activation of the no-wake mode can be  (3) Push the upper side or the lower side of
                            confirmed by the no-wake mode indicator on  the “SPEED  ADJUST” switch  to adjust
                            the multifunction information center.    the engine speed to three settings: “No
                                                                     Wake –1”, “No Wake” (standard setting),
                                                                     and “No Wake +1”.

                                            RPM
                                            x1000
                                                   MPH
                                         No Wake  +1

                              14.3V
                                            1    2
                              1 No-wake mode indicator                                    1
                              2 No-wake mode level
                            To activate the no-wake mode:          1 “SPEED ADJUST” switch
                            (1) Shift into neutral, or release the throttle  To deactivate the no-wake mode:
                                lever and let the engine speed return to  Perform one of the following operations. The
                                idle.                             beeper sounds two times and the no-wake
                            (2) Push and hold the “CRUISE/NO WAKE”  mode indicator  disappears when  the no-
                                switch.  Once the beeper sounds three  wake mode is deactivated.
                                times and the no-wake mode indicator is   Push the “CRUISE/NO WAKE” switch.
                                                                   Squeeze the throttle lever.
                                                                   Squeeze the RiDE lever.
                                                                  TIP:
                                                                  The no-wake mode is also deactivated when
                                                                  the engine is stopped.

                                                                                                   41

| 42 43 44 45 46 47 48 49 50 51 52 |