Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 78 - LIT-18626-13-05
P. 78

    UF4P11E0.book  Page 72  Friday, October 30, 2020  9:39 AM

                            Pre-operation checks

                            right and left fully turned positions of the jet  locked in place. (See page 32 for adjustable
                            thrust nozzle.                        tilt steering system operation procedures.)

                                                                  EJU43213
                                                                  RiDE lever checks
                                                                  Operate the RiDE lever several times to make
                                                                  sure that operation is smooth throughout the
                                                                  whole range. Also, make sure that the RiDE
                                                                  lever returns automatically to its fully closed
                                                                  position when released.

                              Difference between fully turned posi-
                              tions of jet thrust nozzle (distances A
                              and B):
                                Maximum 5 mm (0.20 in)

                            EJU40363
                            Adjustable tilt steering system checks
                            Operate the adjustable tilt steering system  EJU42181
                            several times to make sure that operation is  Throttle lever checks
                            smooth throughout the whole range. Also,  Operate the throttle lever several times to
                            make sure that the handlebars are securely  make sure that operation is smooth through-
                                                                  out the whole range. Also, make sure that the

                            72

| 73 74 75 76 77 78 79 80 81 82 83 |