Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 80 - LIT-18626-13-05
P. 80

    UF4P11E0.book  Page 74  Friday, October 30, 2020  9:39 AM

                            Pre-operation checks

                                make sure that the engine stops immedi-  EJU32535
                                                                  Fire extinguisher check
                                ately.
                                                                  Check that there is a full fire extinguisher on
                            (4) Restart the engine, and then pull the en-
                                                                  board.
                                gine shut-off cord (lanyard) to  remove
                                the clip from the engine shut-off switch
                                to make sure that the engine stops im-
                                mediately.
                            EJU46060
                            Electric trim system check
                            Turn on the multifunction information center,
                            and then operate the “TRIM/T.D.E.” switch.
                            Check that the jet thrust nozzle moves up and
                            down properly and that the trim setting indi-
                            cator change according to the operation of
                            the switch. (See page 45 for information on  To check the fire  extinguisher, see  the  in-
                            turning on the multifunction information cen-  structions supplied by the fire extinguisher
                            ter without starting the engine and page 37  manufacturer. Always keep the fire extin-
                            for information on the electric trim system.)  guisher secured in the holder with its cover in
                                                                  place.
                                                                  Always carry a fire extinguisher on board. A
                                                                  fire extinguisher is not  standard  equipment
                                                                  with this watercraft. If you do not have one,
                                                                  contact a Yamaha dealer or a fire extinguish-
                                                                  er dealer to obtain one meeting the proper
                                                                  specifications.
                                                                    Fire extinguisher:
                                                                      Classification:
                                                                        5-B (B-1)
                            EJU40102                                  Capacity:
                            Storage compartment checks
                                                                        2 lb or more
                            Make  sure that  the storage compartments
                            are not damaged and that water has not col-  EJU40122
                            lected in the compartments. (See page 57 for  Safety equipment check
                            information on the storage compartments.)  Check that safety equipment meeting the ap-
                            EJU43800                              plicable regulations is on board.
                            Fire extinguisher holder, cover, and band   EJU32353
                            checks                                Hull and deck check
                            Make sure that the fire extinguisher holder,  Check the hull and deck for damage or other
                            cover, and band are not damaged and that  problem.
                            the fire extinguisher is securely held in place  EJU32657
                                                                  Jet intake checks
                            using the band. (See page 59 for information  Make sure that the jet intake is not damaged
                            on the fire extinguisher holder, cover, and  or clogged with weeds or debris. If the jet in-
                            band.)                                take is clogged, clean it. (See page 103 for in-

                            74

| 75 76 77 78 79 80 81 82 83 84 85 |