Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 36 - LIT-18626-13-05
P. 36

    UF4P11E0.book  Page 30  Friday, October 30, 2020  9:39 AM

                            Control function operation

                            EJU31027                              (3) Input each digit of the 4-digit PIN, and
                              Watercraft control functions
                                                                     then push the “OK” button of the touch-
                            EJU45091
                            Yamaha Security System                   pad control.
                            The  Yamaha  Security System functions to
                            help prevent unauthorized use or theft of the
                                                                                Enter PIN
                            watercraft. The lock and unlock modes of the
                            security system can  be selected  using  the       * * * *
                            engine lock screen of the multifunction infor-  1      2       3
                            mation center. The engine cannot be started    4       5       6
                            if the lock mode of the security system is se-  7      8       9
                            lected. The engine can only be started if the          0
                            unlock mode is selected.
                            TIP:
                            The  Yamaha Security  System setting  can  TIP:
                            only be selected while the engine is stopped.  The default setting for the PIN is “1234”. The
                            EJU45870                              PIN can also be changed. (See page 49 for in-
                            Yamaha Security System setting        formation on changing the PIN.)
                            The Yamaha Security System setting can be
                                                                  (4) To select the lock mode of the Yamaha
                            confirmed by the lock or unlock mode indica-
                                                                     Security System, select “ON”. To select
                            tor on the multifunction information center.
                                                                     the unlock mode, select “OFF”.
                                                           1
                                                                              Engine Lock
                                                                                  ON
                                                           2
                                                                                  OFF

                              1 Lock mode indicator
                              2 Unlock mode indicator             (5) The beeper sounds once when the lock
                                                                     mode of the Yamaha Security System is
                            To  select the lock or unlock mode of the
                                                                     selected, and two times when the unlock
                            Yamaha Security System:
                                                                     mode is selected.
                            (1) Stop the engine.
                                                                  EJU46112
                            TIP:                                  Engine start/stop switch “  / ”
                            The multifunction information center is turned  ECJ01311
                            on, even if the engine start/stop switch is also
                            pushed briefly.                       Do not run the engine over 4000 r/min on
                            (2) Select the lock or unlock mode indicator  land. Also, do not run the engine for more
                                on the multifunction information center.

                            30

| 31 32 33 34 35 36 37 38 39 40 41 |