Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 39 - LIT-18626-13-05
P. 39

    UF4P11E0.book  Page 33  Friday, October 30, 2020  9:39 AM

                                                             Control function operation

                            To adjust the handlebar position:     (2) Make sure that the tilt lever returns to its
                            (1) Pull the tilt lever up to disengage the han-  original position and that the handlebars
                                dlebar lock, and then move the handle-  are securely locked in place.
                                bars back or forth to the desired position.
                                WARNING! Never pull the tilt lever dur-
                                ing  operation, otherwise the  handle-
                                bars may  suddenly change  position,
                                which may lead to an accident. [EWJ00042]

                                                      1
                                                                  EJU41801
                                                                  Cooling water pilot outlets
                                                                  When the engine  is running, some of the
                                                                  cooling water that is circulated in the engine
                                                                  is discharged from  the cooling  water pilot
                              1 Tilt lever                        outlets.

                                                                            1
                                                                   1 Cooling water pilot outlet
                                                                  There are cooling water pilot outlets on the
                                                                  port (left) and starboard (right) sides of  the
                                                                  watercraft. To check for proper operation of
                                                                  the cooling system, make sure that water is
                                                                  being discharged from the port (left) pilot out-
                                                                  let. If water is not being discharged from the
                                                                  outlet, stop the engine and check the jet in-
                                                                  take for clogging. (See page 103 for informa-
                                                                  tion on the jet intake.)

                                                                                                   33

| 34 35 36 37 38 39 40 41 42 43 44 |