Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 68 - LIT-18626-13-05
P. 68

    UF4P11E0.book  Page 62  Friday, October 30, 2020  9:39 AM

                            Operation and handling requirements

                            (4) Loosen the fuel filler cap and remove it.  Do not  leave the watercraft with  a full
                                                                     tank in direct sunlight.

                                                         1

                                                                                               1

                              1 Fuel filler cap
                            (5) Slowly add fuel to the fuel tank.  1 Top of the fuel tank

                              Fuel tank capacity:                                           1
                                70 L (18.5 US gal, 15.4 Imp.gal)                                 2

                                                                   1 Top of the fuel tank
                                                                   2 Approximately 50 mm (2 in) from top of the
                                                                     fuel tank
                                                                  (7) Wipe up any spilled fuel immediately with
                            (6) Stop filling  when the  fuel level reaches
                                                                     a dry cloth.
                                approximately 50 mm (2 in) from the top
                                                                  (8) Securely install the fuel filler cap by tight-
                                of the fuel tank. Do not overfill the fuel
                                                                     ening it until it clicks.
                                tank. Because fuel expands when it
                                                                  (9) Securely install the seats in their original
                                heats up, heat from the engine or the sun
                                                                     positions.
                                can cause fuel to spill out of the fuel tank.

                            62

| 63 64 65 66 67 68 69 70 71 72 73 |